
Town of Farmersville
Building Code Enforcement

Procedure for Demolition of Buildings
· Submit contractor workers compensation and liability insurance. If being done by owner, NYS Workers Comp. CE-200 waiver is required
· Survey, plot plan, sketch of property showing relative location of building(s) to be demolished
· You must verify that utilities are disconnected
· Date & person contacted

· Gas/propane/oil
· Water/well
· Sewer (Town Hall) or Septic (Catt Co. Health Department)
· National Grid
· Telephone
· Cable
· Other
· Property owner or contractor has been advised that it is their responsibility for compliance with the NYS Labor Department Industrial Code Rule 56 – Asbestos, lead paint, other hazardous material.
· All excavations, holes, depressions must be filled to grade with clean compacted fill

· All above or below ground tanks must be properly emptied, cleaned, and removed

· All rubble, debris, etc. must be removed from the site and properly disposed…NOT BURIED!

· Safety during demolition must conform to Section 3303 of the 2020 Building Code of NYS
Applicant acknowledgement
Signiture:_____________________________
Date:_____________
